



|  |  |  |
| --- | --- | --- |
| **Reach Layout** | **SMALL STREAMS** | **LARGE STREAMS** |
| (average wetted width less than or equal to 4.0 m) | (average wetted width greater than 4.0 m) |
| Transect (Flow, Cross Section, Canopy Cover) | **5 Lettered Transects spaced 40 meters apart** | **5 Lettered Transects at 10X average wetted width apart** |
| Example: | Example: |
| Average wetted width = 3m | Average wetted width = 6m |
| Distance between transects = 40m | Distance between transects = 60m |
| Total Reach Length = 160m | Total Reach Length = 240m |
| Transect A (1st transect) = 0 meters | Transect A (1st transect) = 0 meters |
| Transect E (5th transect) = 160 meters | Transect E (5th transect) = 240 meters |
| Intermediate Transect (Pebble Count) | **21 Contiguous Transects spaced 8 meters apart** **(i.e., entire reach layout)** | **21 Contiguous Transects at 2X average wetted width (i.e., entire reach layout)** |
| Example: | Example: |
| Average wetted width = 3 | Average wetted width = 6 |
| Distance between intermediate transects = 8 | Distance between intermediate transects = 12 |
| Total Reach Length = 160 | Total Reach Length = 240 |
| Thalweg Profile Stations | **Measure thalweg depth every 1.0 meter (160 total measurements)** | **Measure thalweg depth at intervals equal to total reach length divided by 160 (160 total measurements)** |
| Example: | Example: |
| Average wetted width = 3 | Average wetted width = 6 |
| Distance between profile stations = 1 | Distance between profile stations = 1.5 |
| Total Reach Length = 160 | Total Reach Length = 240 |
| Total measurements = 160 | Total measurements = 160 |













 





